|  |  |
| --- | --- |
| **Solar Ribbon Stringing with Epoxies** | |
| [https://www.epotek.com/site/images/brochures/thumbnails/SAS_Solar_Ribbon.jpg](https://www.epotek.com/site/files/brochures/pdfs/SAS_Solar_Ribbon.pdf) | Solar ribbons can be attached with Silver-filled epoxy, often referred to as Electrically Conductive Adhesives (ECAs), as well as other conductive joining materials including, solder and Pressure Sensitive Adhesives (PSA) tapes. Solder joining ribbons to TCO/PV layers is the mainstream process used with crystalline Si wafer cells. |