|  |
| --- |
| **Solar Ribbon Stringing with Epoxies** |
| https://www.epotek.com/site/images/brochures/thumbnails/SAS_Solar_Ribbon.jpg | Solar ribbons can be attached with Silver-filled epoxy, often referred to as Electrically Conductive Adhesives (ECAs), as well asother conductive joining materials including, solder and Pressure Sensitive Adhesives (PSA) tapes. Solder joining ribbons to TCO/PV layers is the mainstream process used with crystalline Si wafer cells. |